Example 1:

sample:		calcite (10.4)-water interface
instrument:	Bruker Nanoscope V
type:		dynamic AFM

Analysis Parameters:

module:		periodic structures
algorithm:	algorithm 1

mode:		auto-correlation
anal. area	full image
max order	3
order filt.	individual
max period.	/
spot radius	0.3e-9 m
spot threshold	0.3
lat. tol.	0.15
init. guess.	closest
marker spots	5
matching	none

Note: Results of the retrace images are erroneous due to spurious peaks caused by noise.

Calibration Parameters:

"kX": 1.14,
"dkX": 0,
"kY": 0.99,
"dkY": 0,
"beta": 89.7,
"dbeta": 0