Example 1:

sample:		calcium fluoride (111) in UHV
instrument:	Omicron Matrix AFM
type:		dynamic AFM

Analysis Parameters:

The data can be analyzed with the standard parameters.

module:		periodic structures
algorithm:	algorithm 1

mode:		auto-correlation
anal. area	full image
max order	3
order filt.	individual
max period.	/
spot radius	0.1e-9 m
spot threshold	0.3
lat. tol.	0.15
init. guess.	closest
marker spots	5
matching	brute force (lattice vectors)

Calibration Parameters:

"kX": 0.8184,
"dkX": 0,
"kY": 0.893,
"dkY": 0,
"beta": 88.39,
"dbeta": 0